# Deployment

The deployment of the NetSpective solution typically takes between 90 minutes to no more than 4 hours. The deployment model for a typical customer goes as follows.

* The NetSpective appliance is unboxed and rack mounted.
* The appliance is licensed and given an IP address.
* The NetAuditor software is installed on a local server or VM.
* Through the remote assistance of TeleMate.Net Software, the following will be configured;
  + LDAP is integrated to populate NetSpective with users and groups.
  + Basic policy is created and assigned to users.
  + We cover authenticating users though the various devices the district uses.
  + Configure NetSpective to send logs to NetAuditor.
  + Any additional training on either product is covered.
* Network diagrams for both local and remote deployments are provided on the next page.